[viewBag] title = "MOBILE NVR WITH AI" url = "/solutions/mobile-nvr-ai" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# MOBILE NVR WITH AI

## Description

NVR (Network Video Recorder) is a video recording system over network, commonly used for surveillance and security purposes. This device streams security video footage from IP cameras and records the footage in digital format on to a sata hard drive. NVRs Uses wired or wireless network to connect to IP cameras. Streams are transferred using TCP or UDP protocol.

## Features

- Runs Linux Kernel 5.10 with Yocto Root File System (RFS).
- Streams video from IP cameras over wired network that can be configured upto 16 channels.
- Uses Real Time Streaming Protocol (RTSP) based on client server architecture.
- Uses H.264, H.265 decoder and wayland sink for rendering
- Simultaneously stores streamed data onto hardisk through SATA interface.
- Uses open source GStreamer plugins pipeline to parse and decode the RTSP Packets.
- Capable of rendering videos from 16 tiles onto single window that can be monitored over HDMI Interface.
- Can be used for basic analytics by running Neural Network model on Deepx NPU
- Supports QT for GUI application developement.
- Supports scaling.
- MCU with OTP area for network MAC ID
- 6-Port USB smart hub with: - Five standard USB 3.2 Gen 2 downstream ports. - One standard USB 2.0 downstream port.
- It uses all automotive type connectors.
- Operating input volatage: 18-24VDC
- Battery-14.8V, 2000MHz, 3hr.
- MAC ID storing and secure chip.
- Magnetics on board.
- Audio codec DA7218 for 2mics.
- Stereo jack speaker out.
- PCIE interface for NVME SSD and DEEPX
- PCIE to SATA connection through SATA expansion controller adapter card.
- HDMI out.
- Display HDMI / LVDS with cap touch.
- 1Gbps Ethernet.
- USB 2.0, USB 3.0 with NVME SSD and 4G/5G module USB 2.0 connected USB hub of USB 2.0
- 8 GPIO non isolated pins.
- 2 UART RS232 ports, 1 CAN 2.0B, 2 RS485, 2 IDC ports, GPIO isolated port

##

## Software Environment

- Host setup: Ubuntu 20.04 LTS.
- Open source GStreamer version 1.0
- Yocto SDK RZ/G Verified Linux Package (VLP) for 64 bit kernel, BSP version 3.0.x S
- ftware stacks supported:
- - Web browser: Firefox.
- - Web server: Apache / Lighttpd.
- - Backend script: PHP.
- - RDBMS support: MySQL / SQLite.

## Applications

- Public safety.
- Traffic monitoring.
- Industrial monitoring.
- Video surveillance for locomotives like Train, Bus, truck
- Mobile NVR
- Commercial NVR

## Block Diagram