[viewBag] title = "LTCT METER" url = "/solutions/ltct-meter" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# LTCT METER

#

##

## Description

Low Tension Current Transformer Meter (LTCT) is Used To Record Power Consumption Of Loads Ranging From 26 kW to 99 kW. It Is A Combination Of A Current Transformer (CT) and an Energy Meter. LTCT Meters Are Highly Accurate And Reliable.

## Features

- Meter Accuracy : Class - 1
- Base Currrent : 1A / 5A
- Max Current : 30A
- Auxillary Supply : 120V - 240V AC
- Communication : RS485 (Modbus PProtocol)
- Harmonics : Detects upto 21st Harmonics

## Applications

- Renewable Energy Applications
- Industrial Settings
- Smart Grid Systems
- Commercial Settings

## Block Diagram