[viewBag] title = "SEQUENTIAL LED INDICATOR" url = "/solutions/sequential-led-indicator" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# SEQUENTIAL LED INDICATOR

## Description

The Sequential LED Indicator Demonstrated Here Is Built Around Renesas RL78-F12 Microcontroller, and Taiwan Semiconductor CCR For Individual Light Control.

## Features

- Simple & Robust Design
- Operating Voltage: 10V-21V
- LED Current Upto 200mA
- Battery Reverse Protection
- Sequential Time Can Be Adjustable Easily
- Production Friendly Compared To Analog Sequential To Match The Sequence Time
- No Of Sequence Can Be Added Upto 16
- Sequential Animation Can Be Alter Easily
- Synchronise Can Be Done For Front And Rear Indicator

## Applications

- Automotive lighting
- Safety and warning systems

##