[viewBag] title = "RA6M4 MCU / EBN CLUSTER" url = "/solutions/ra6m4-smart-cluster" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 banner = "/Solutions/solution-banner.jpeg" ==

# RA6M4 MCU / EBN CLUSTER

#

## Description

The 2-wheeler smart cluster integrates technology, connectivity, and intelligent functionalities to deliver an enriched riding experience. This design has wireless module for communicating with smartphones.

It provides essential data, connectivity choices, and safety elements, all within a streamlined and user-friendly interface tailored specifically for motorcycles. With these features it transforms a traditional cluster into a smart one.

## MCU

MCU | Renesas RA6M4 - 100Pin 1MB Flash/256KB RAM / 8KB Data Flash
CORE | Cortex M33

##

## Connectivity

BLUETOOTH | Dialog DA14531 - BT 5.1
GSM | Quectel LTE Module
GNSS | GPS GLONASS or GPS IRNSS

##

## Hardware

LCD | 5"/7" EBN Display
MEMORY | QSPI Flash 64MB
DISPLAY | EBN Module with 12C Interface
GSM INTERFACE | UART
CAN (BD41041FJ) | AEC-Q100 Qualified Transmission Rate of 40kbps to 1Mbps
BLUETOOTH (DA14531) | UART Interface
ALS | Ambient Light Sensor with IR LED
USIM | x2, Support 1.8/2.95V (U)SIM Cards, with (U)SIM Card Detection Function
GYRO & ACCELEROMETER (LSM6DS3TR) | 16-bit Digital Triaxial Accelerometer And Gyro Sensor

##

## Software

Renesas RA6M4 | IDE E2 Studio/E2 Studio, Azure RTOS, FREE RTOS
Dialog | Keil, IDE

##

## Block Diagram