[viewBag] title = "SMART CLUSTER SC200R" url = "/solutions/smart-cluster-sc200r" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# SMART CLUSTER SC200R

## Description

The Smart Cluster reference solution is a complete cluster system featuring a capacitive touch display for quick navigation, an odometer, light indicators, tire pressure readings, maps, and an area for displaying custom logos.

This design has also been upgraded with wireless capabilities for connecting to smartphones, transforming a traditional cluster into a smart one.

## GPU and CPU

GPU | Qualcomm Adreno™ 308 Graphics Processing Unit with 64-bit addressing
CPU | QCM2150, Quad-core ARM Cortex-A53 64-bit CPU @ 1.3 GHz

## Connectivity

BLUETOOTH | BT 4.2 (BR/EDR + BLE)
GNSS | GPS/ BeiDou / GLONASS or GPS/ BeiDou /Galileo
WI-FI | 2.4/5 GHz dual-band WLAN based on IEEE 802.11a/b/g/n, up to 150 Mbps

## Hardware

LCM | × 1, 4-lane MIPI_DSI, HD+ (1440 × 720) @ 60 fps
MEMORY | 1 GB LPDDR3 + 8 GB eMMC | 2 GB LPDDR3 + 16 GB eMMC
DISPLAY | 4 lane MIPI_DSI; HD+ HD+(1440*720) @60fps
TOUCH PANEL | Capacitive touch panel
CAMERA | 2 groups of 4 lane MIPI_CSI, up to 2.1Gbps per lane Support 2 or 3 cameras, up to 13 MP with dual ISP
AUDIO | 3 analog inputs: MIC1, MIC2, MIC3 3 analog outputs: speaker, earpiece, headphone
VIDEO | Video encoding + decoding: 720p @ 30 fps + 1080p @ 30 fps Encoding up to 1080p @ 30 fps, decoding up to 1080p @ 30 fps
USB 2.0 | × 1, compliant with USB 2.0, support USB OTG, USB OTG + charge, etc.
SD CARD | × 1, SD 3.0, support 4-bit SD mode
CAN | AEC-Q100 Qualified transmission rate of 40kbps to 1Mbps
ALS | Optical proximity and ambient light sensor with IR LED
USIM | x2, Support 1.8/2.95V (U)SIM cards, with (U)SIM card detection function
GYRO & ACCELEROMETER | 16-bit digital triaxial Accelerometer and Gyro Sensor
SERIALIZER | Supports MIPI CSI-2 data transmission
UART | Support 4Mbps, one of them supports Hardware Flow Control
DIMENSIONS | Module:- 40.5mm*40.5mm

## Software

ANDROID | Operating System version 10
LINUX | Kernel version 4.9.218

## Block Diagram