[viewBag] title = "SEQUENTIAL LIGHTING" url = "/solutions/sequential-lighting" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# SEQUENTIAL LIGHTING

##

## Description

Sequential LED Indicator Demonstrated Here Is Built Around Renesas RL78-F13 Microcontroller, and Melexis MLX81115 CCR For Individual Light Control.

The MLX81115 LIN RGB slave provides a single chip solution for driving up to six LEDs via constant current sources in automotive ambient lighting applications. Every output can be programmed to a maximum current of 48 mA through the built-in Flash memory.

## Features

- Simple & Robust Design.
- Operating Voltage: 10V-21V.
- LED Current Upto 200mA.
- Battery Reverse Protection.
- Sequential Time Can Be Adjustable Easily
- Production Friendly Compared To Analog Sequential To Match The Sequence Time
- No Of Sequence Can Be Added Upto 16.
- Sequential Animation Can Be Alter Easily.
- Synchronise Can Be Done For Front And Rear Indicator

## Applications

- Automotive Lighting
- Safety and Warning Systems

##

## Block Diagram