[viewBag] title = "RZ/G2L ANDROID / LINUX CLUSTER" url = "/solutions/rz-g2l-android-linux-cluster" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# RZ/G2L ANDROID / LINUX CLUSTER

## Description

An Android Cluster is a digital dashboard powered by the Android operating system, commonly used in vehicles, including two-wheelers. It provides real-time data such as speed, navigation, diagnostics, and smartphone connectivity, enhancing rider convenience and safety.

## Features

- Processor – General-Purpose MPU with Dual-Core Arm Cortex-A55 CPUs and Single-Core Cortex-M33 CPU with 3D Graphics and Video Codec Engine
- eMMC 32GB
- DDR4 2GB (4GB optional)
- SD Card Interface
- 7’’ TFT LVDS Interface – Touch CTP
- ALS Ambient Light Sensor – RTR-0521RS
- GSM - LTE EC800K
- GPS, BDS, Gallieo and GLONASS
- Wifi 5 + BLE BT5.0
- BLE Standalone - DA14531(Optional)
- Audio Codec - DA7218 Stereo Codec with Single ended headphone driver
- Accelero and Gyro - SMI230
- MIPI Camera AHL Interface (Encoder RAA279971 and Decoder RAA279972)
- CAN Interface RL78/F14 - UART output for RZ/G2L
- CAN Communication: OBD Interface, BMS, etc…
- Hardware Indicators (Left/Right Turn)
- Side Stand Indicator
- Head Light Switch
- Throttle Pulse/ADC

## Block Diagram