[viewBag] title = "IRIS AND FPS" url = "/solutions/iris-and-fps" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# IRIS and FPS

#### L1 COMPATIBLE

#

##

## Description

IRIS(Eye) and Fingerprint Sensors are biometric technologies used for identification and authentication purposes. an IRIS sensor captures the unique patterns of the iris can be used to identify individuals with a high level of accuracy. Fingerprint sensors use capacitive or optical technology to capture the unique patterns on the fingertips.

This solution rely on biometric data, which is a unique characteristic of an individual that can be used to identify them. When the IRIS and FPS systems grant access, a signal is sent to a microcontroller that is connected to the TFT display.

##

## Features

- RZ/A2M (324 Pin BGA).(R7S921058VCBG)
- MIPI CAMERA (MT9V034LCC)
- Quad SPI (MX25L51245G-M-SOP16P)
- USB 2.0 WITH CDC Interface
- USB 2.0 is Host Interface
- Intersil Buck Regulator(ISL80505,ISL80030A)
- Buzzer Interface
- Indication Tri Color LED
- IR LED Control
- FPS Sensor Interface
- 2.8inch TFT Display

## Applications

- Access Control
- Time And Attendance
- Law Enforcement
- Healthcare

##

## Block Diagram