[viewBag] title = "USB PD CHARGER 65W" url = "/solutions/usb-pd-charger-65w" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# USB PD CHARGER 65W

## Description

65W Buck Boost is a high-efficiency synchronous Buck-Boost controller with IIC/FB. It allows the realization of a Buck-Boost converter with only one inductor and power MOSFETs. It supports input voltage range of 5V~36V and output voltage range of 3V~21V, and output voltage can be regulated by IIC or FB. It has a fully integrated Type-C / PD and DPDM fast charge controller. It complies with the latest Type-C and PD 3.1 standards and supports the most popular high voltage fast charge protocols with DPDM interface and targets for automotive charger applications.

## Block Diagram

## Applications

- Car USB charger
- Automotive power charging applications

##

## Features

- AEC-Q100 Qualied for Automotive Applications:

» Temperature Grade 2: -40°C~+105°C

- Integrate USB Power Delivery (PD2.0/PD3.1):

» USB Type-C/PD protocol

» Auto-detect Type-C attach and detach

» Support USB PD2.0/PD3.1/PPS

» VCONN and SDO/P supported for e-mark

- Private Protocols

» Xiaomi’s private charging protocol

» OPPO’s private charging protocol

- Fast Charge

» Support QC2.0/QC3.0/QC4/QC4+

» Support AFC and Class B

» Support Huawei FCP protocol

» Support Huawei SCP protocol

» Support MTK PE1.1/2.0 protocol

» Support MTK’s AFC fast charge protocol

- PE 2.0: 5V/9V/12V/15V

- PE+ 11: 5V, 9V, 12V

» Support BC1.2, Apple 2.4A, Samsung* 2.0A

- Auto detection Voltage and Signals on CC1, CC2 and DP, DM For Dierent Fast Charge

» Support USB-A and Type-C dual port output

» Fast charge single port output and 5V for dual port output

- Power Management

» A DC port 5V output

» Support ADOE mode

» Built-in power path management

» Dynamic port priority function

» Support auto-detecting flow mode

- Multiple Protection, High Reliability

» OVP overvoltage protection and short circuit protection

» NTC temperature protection

» DPDM/CC1/CC2 overvoltage protection

» DPDM short circuit with OVP delay protection

» DP/DM input OVP to 30V

» CC1/CC2 input voltage up to 30V

- Built-in 2kbit OTP-ROM

» Flexible customization: software, supporting up to three upgrades

- Working voltage: 3V~30V
- Package QFN24 (4mm4mm0.75mm)