[viewBag] title = "TARJANI MODULE" url = "/solutions/tarjani-module" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# TARJANI MODULE

#

## Description

Tarjani Module was used for POC for Aadhaar- L1 application to support PCH certification for renesas synergy controller.

## Features

- USB Powered
- Reliable Capturing Performance
- Sleek And Stable Design
- High-Quality Certified FMR Extractor
- S5D9 – R7FS5D97C2A01CBG#AC0,176-Pin BGA package,120 MHz Arm® Cortex®-M4 core with Floating Point Unit (FPU),640 KB SRAM,1MB Code Flash Memory,8 Kb Data Flash Memory.
- Build around BIOSEC capacitive area sensor with array 365 by 256
- Support for USB-2.0 (HS/FS) For Easy Connectivity
- Compatible with Various HOST-Environment: Linux, MS-Windows, iOS and Android
- 508 dpi (256 x 365 pixels), 256 Gray Level Sensor
- Hardware Encryption Support @ RSA-2048 bit Key-Generation and AES-256 bit
- Secured With No-availability For JTAG Interface (Hardware Disabled)
- Secure Updates Only Available Via Secure Boot-loader After Authentication

##