[viewBag] title = "IRIS WITHOUT TFT" url = "/solutions/iris-without-tft" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

## IRIS WITHOUT TFT

## Description

IRIS (eye) and fingerprint sensors are biometric technologies used for identification and authentication purposes. An IRIS Sensor captures the unique patterns of the iris can be used to identify individuals with a high level of accuracy. This solution rely on biometric data, which is a unique characteristic of an individual that can be used to identify them.

## Features

- RZ/A2M (256 Pin BGA), R7S921056VCBG
- MIPI CAMERA (MT9V034LCC)
- Quad SPI (MX25L51245G)
- USB 2.0 WITH CDC Interface
- Intersil Buck Regulator (ISL80505, ISL80030A)
- Buzzer Interface
- Indication Tri Color LED
- IR LED Control

## Applications

- Access Control
- Time And Attendance
- Law Enforcement
- Healthcare