[viewBag] title = "RA6M3 MCU / TFT CLUSTER" url = "/solutions/ra6m3-smart-cluster" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 banner = "/Solutions/solution-banner.jpeg" ==

# RA6M3 MCU / TFT CLUSTER

## Description

The 2-Wheeler Smart Cluster integrates technology, connectivity, and intelligent functionalities to deliver an enriched riding experience. This design has wireless module for communicating with smartphones.

It provides essential data, connectivity choices, and safety elements, all within a streamlined and user-friendly interface tailored specifically for motorcycles. With these features it transforms a traditional cluster into a smart one.

## MCU

MCU | RenesasRA6M3-176Pin2MBFlash/640KBRAM/64KBDataFlash
CORE | CortexM4

##

## Connectivity

BLUETOOTH | DialogDA14531-BT5.1
GSM | QuectelLTEModule
GNSS | GPSGLONASSorGPSIRNSS

## Hardware

TFT | 5" TFT 800 X 480
MEMORY | SDRAM - 64MBytes, QSPI Flash 64MB
DISPLAY | 16bit RGB
GSM INTERFACE | UART
CAMERA | 1Ch - Analog Composite Video Inputs
RPS | RPS - Rear Vision Video Display For Reverse Parking
CAN (BD41041FJ) | AEC-Q100 Qualified Transmission Rate of 40kbps to 1Mbps
BLUETOOTH | UART Interface
GYRO & ACCELEROMETER (LSM6DS3TR) | 16-bit Digital Triaxial Accelerometer And Gyro Sensor
ALS | Ambient Light Sensor with IR LED
USIM | x2, Support 1.8/2.95V (U)SIM Cards, with (U)SIM Card Detection Function

##

## Software

Renesas:IDEE2Studio/E2Studio,AzureRTOS,FREERTOS
GUI:Sparklite,GUIX,Seggerwin

##

## BlockDiagram

##