[viewBag] title = "INDUSTRIAL POE 24-PORT SWITCH" url = "/solutions/industrial-poe-24-port-switch" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# INDUSTRIAL POE 24-PORT SWITCH

##

## Description

Robust unmanaged industrial Ethernet switches with M12 connectivity for use in railways and other forms of public transport. This is designed for industrial applications in harsh environments. The M12 connectors ensure tight, robust connections, and guarantees reliable operation, even for applications that are subject to high vibration and shock.

## Features

- M12 connector with A-Coded 8 Pin or X-Coded Connectors.
- Unmanaged Switch Has MCU & EEPROM to Disable Ports On The Fly
- Provides 24 fast Ethernet ports with Auto MDI/MDI-X Supports 10/100 Mbps auto-negotiation.
- All M12 ports with IEEE 802.3af compliant PoE ports, The switch is classified as power source equipment (PSE) and provide up to 15.4/30 W of power per port.
- Ethernet switch supports IEEE 802.3/802.3u/802/3x with 10/100M, full/half-duplex, MDI/MDI-X auto-sensing, and provides an economical solution for your industrial Ethernet network.
- Each port supports both 10/100 Mbps speed auto negotiation.
- Standards: IEEE 802.3 for 10BaseT, IEEE 802.3u for 100BaseT(X), IEEE 802.3x for Flow Control Processing.
- Type: Store and Forward Flow Control: IEEE 802.3x full duplex, back pressure flow control.
- Supports redundant 110V + 30%
- 150WATT total power.
- LED Indicators Power 1, Power 2 10/100T (X): Link/Activity.
- Automatic MDI/MDI-X crossover for plug-and-play Store-and-forward architecture Auto-detection of PD (powered devices) and automatic power management (NSM-208PSE-M12-IP67).

##

## Applications

- Public Transportation - Buses, Ambulances
- Railway
- Heavy Industrial Applications
- Metros

## Block Diagram