[viewBag] title = "RDAS CAMERA" url = "/solutions/ip-camera" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# RDAS CAMERA

#

## Features

- RZ/V2L with Integrated Secure element which Features:
  - Tamper resistance,
  - Unlimited secure key storage,
  - Hardware cryptographic acceleration (RSA),
  - SPA/DPA resistance,
  - Isolation technologies including Arm® TrustZone®
  - Device Lifecycle Management
- Fish eyes de-warping
- Videos can be saved to the micro SD card
- Provide Onvif protocol
- IR build in
- Support WebRTC interface
- Interface standard: ONVIF Profile S, CGI
- AI: Human detection/ Motion detection

## Specifications

- Sensor: Omnivison OS02G10 2MP, 1/2.9" Optical Format, 1080P, 30 FPS
- Encoder: H.264
- White Balance: Auto, Manual
- LAN: RJ-45 (10/100Base-T )
- WIFI on board
- RTC: built-in & Time Storage
- Audio: Sound format, Support MIC Input
- Power Supply: DC 12V(2A), POE(Optional)
- Consumption: <3W(Max)

## Block Diagram

##