[viewBag] title = "RL78 CLUSTER" url = "/solutions/rl78-cluster" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# RL78 CLUSTER

##

## Description

Renesas's reference solution for Smart Cluster includes a full cluster functionality with additional features for dashboard market segments. There are various key features such as stepper motor for RPM & Segmented LCD display for Speed. Renesas's automotive grade RL78/D1A 16-bit microcontrollers series contains flash memory from 24K-512K and possess a wide range of packages that supports 48-128 pins. The reference solution possess CAN bus interface, sound generator interface, stepper motor with ZPD and LCD segment. Renesas provides easy hands on development tools, making development process easier than you have ever imagined.

## Features

- Addition Bluetooth wireless modules to communicate with smart phone for functionalities such as Diagnosis, Navigation, etc
- Stepper motor RPM & LCD for Speed & other indications like odometer, trip, RTC, Fuel, etc. are available
- Provision for connecting ZigBee wireless modules
- Wide range of interface support: CAN bus interface, sound generator, stepper motor, etc
- RL78/D1A 16-bit True Low Power microcontroller

- 32 MHz flash memory/RAM up to a maximum of 512 KB/24 KB

- CAN or LIN interface

- Stepper motor controller/driver

- Up to 216 segment LCD controller/drive.

## Block Diagram

##