[viewBag] title = "7\" INDUSTRIAL TABLET" url = "/solutions/android-tablet" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 banner = "/WhatsApp Image 2024-09-26 at 11.09.53 AM.jpeg" ==

# 7" INDUSTRIAL TABLET

#

# Description

Industrial Android Tablets combine the user-friendly features of Android with rugged durability, representing a significant technological advancement that enhances efficiency and productivity in demanding industrial environments.

##

## Features

- Processor - The RZ/G2L microprocessor includes a Dual Core - Cortex®-A55 (1.2GHz) CPU
- Memory –

- eMMC – 64GB / 128GB

- DDR4 – 4GB / 8GB

- SD CARD
- Display – 5.5” 720 X 1280 / 7” 800 X 1280, CTP
- HDMI Output
- Camera – MIPI interface
- Audio Codec – DA7218
- Power – main battery: li-ion, rechargeable, 8000 mAh
- USB PD fast charging with Dual Cell Battery
- High Brightness Automotive Grade TFT with Cover Glass
- Interface – 4 ports USB 2.0 Type-C, OTG
- Navigation – GPS (RTK/DR) LC29HDA
- Communication:

- Isolated RS485

- Isolated RS232

- Isolated SPI

- Isolated CAN

- Connectivity:

- 10/100 ethernet (IC Plus)

- Quectel LTE (EC200U)

- Wi-Fi + BLE (FCM360W)

- Sensors:

- Accelero/gyro

- Temperature/humidity

- ALS

- Secure – NFC receiver - PTX100R NFC Reader IC, EMVCo® 3.0/3.1 PCD L1 compliancy2
- Front Camera: 5MP
- Rear Camera: 13MP
- Inbuilt QR CODE READER: Zebra SE4710 - 1D,2D/QR Codes (including AADHAAR).
- LORA Connectivity

#

## Applications

- Inventory management
- Asset management
- Health and safety monitoring.
- Real-time communication

##