[viewBag] title = "KEY FOB" url = "/solutions/key-fob" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 banner = "/Key Fob.jpg" ==

# KEY FOB

## Description

One of the primary functions of a BLE key fob is to remotely lock and unlock the two-wheeler's ignition or steering lock, providing a convenient way to secure the vehicle without needing to insert a physical key.

## Features

- Dialog DA14531 low energy BLE5.0 module
- Battery: CR2032
- Lifetime: 2 years
- Frequency: 2402/2426/2480 MHz
- Broadcasting protocol: iBeacon
- Broadcasting interval: programmable
- Broadcasting power: 0DBm as default, programmable
- Antenna: PCB
- Distance: < 50 meters
- Working power supply: 1.7 ~3.6V DC

##

##