[viewBag] title = "FPS EVK MODULE" url = "/solutions/fps-evk-module" layout = "page-solutions" is_hidden = 0 navigation_hidden = 0 ==

# FPS EVK MODULE

#

## Description

The Tarjani – Evaluation Kit (EVK) V1 enables developers to get started with initial firmware development for finger print sensor (FPS) L1 certification. The major components of EVK – V1 consists of Renesas microcontroller and Biosec FPS Module enabled for multiple sensor interface (i.e SPI, PDC and parallel port).

## Features

- S5D9 – R7FS5D97C2A01CBG#AC0
- 176-Pin BGA package
- 120 MHz Arm® Cortex®-M4 core with Floating Point Unit (FPU)
- 1MB code flash memory, 8 KB data flash memory
- 2D capacitive fingerprint area sensor
- Sensor array of 360 by 256 pixels
- 508 DPI spatial resolution
- Image capture speed up to 2 MPixel/sec
- Low power : Normal and Standby modes
- 30 million finger placement

##

##